**Sea\_Surface\_Temperature**

 Location: 1m

 Manufacturer: SeaBird

 Model: This is either SBE37 or SBE16

 Accuracy: < 0.01 °C

 **Sea\_Surface\_Salinity**

 Location: 1m

 Manufacturer: SeaBird

 Model: This is either SBE37 or SBE16

 Accuracy: < 0.05

 **CO2**

 Measurement Method: Absolute, non-dispersive infrared (NDIR) gas analyzer

 Manufacturer: Licor

 Model: LI-820

 Frequency: 3hr cycle

 Accuracy of CO2water: 2 µatm

 Accuracy of CO2air: 1 µatm

 Precision of CO2water: 0.7 µatm

 Precision of CO2air: 0.6 µatm

 CO2 Sensor Calibration: At the beginning of each sample, the instrument self-calibrates using a zero and high standard. The zero standard is generated by cycling a small amount of air through a soda lime chamber. The high standard is from a cylinder of calibrated standard reference gas from ESRL. ESRL standards are traceable to WMO x93 scale with a stated reproducibility of 0.06 µmol mol-1. For more information on estimates of accuracy and precision of the MAPCO2 system, see Sutton et al. 2014 (reference below).

 Manufacturer of CO2 calibration gases: NOAA Earth System Research Laboratory (ESRL)

 Method References: Sutton, A.J., Sabine, C.L., Maenner-Jones, S., Lawrence-Slavas, N., Meinig, C., Feely, R.A., Mathis, J.T., Musielewicz, S., Bott, R., McLain, P.D., Fought, J., Kozyr, A., 2014b. A high-frequency atmospheric and seawater pCO2 data set from 14 open ocean sites using a moored autonomous system. Earth Sys. Sci. Data, 6, doi: 10.5194/essd-6-353-2014, 353–366.